Information Review Table:

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter/Symbol | Description | Units | Fixed/Derived/Selectable |
| D\_body | Distance from body center of gravity to reference point | Meter(m) | Fixed: 0.18m |
| D\_cone | Distance from cone center of gravity to reference point | Meter(m) | Fixed: 0.04m |
| D\_fins | Distance from center of grav for all fins to reference point | Meter(m) | Fixed: 0.28m |
| SA\_body | Surface area of body | Square Meter (m^2) | Fixed: 0.038485 m^2 |
| SA\_cone | Surface area of cone | Square Meter (m^2) | Fixed: 0.007507 m^2 |
| SA\_fins | Surface area of fins | Square Meter (m^2) | Selectable/Derived |
| Diameter (Diam) | Diameter of rocket | Meter(m) | Fixed: 0.0248m |
| Stability Margin (Stab) | Stability margin of rocket | N/A | Fixed: 2 |
| Center of Gravity (C\_g) | Rocket total center of gravity. Approximated point where gravity will act on the rocket. | Meter(m) | Fixed: 0.2m |
| Center of Pressure (C\_p) | Rocket total center of pressure. If closer to tip than C\_g, will cause spinning | Meter(m) | Derived: (D\_body\*SA\_body+D\_cone\*SA\_cone+D\_fins\*SA\_fins)/(SA\_body+SA\_cone+SA\_fins) |
| Number of Fins (Nfins) | Number of fins, will heavily affect stability, moving C\_p | fins | Selectable |
| CA\_fins | Cross sectional area of fins | Square Meter (m^2) | Derived |
| Fthicc | Fin thickness | Meter(m) |  |